# See: http://code.google.com/p/arduino/wiki/Platforms

##############################################################

uno.name=Arduino Uno
uno.upload.protocol=arduino
uno.upload.maximum_size=32256
uno.upload.speed=115200
uno.bootloader.low_fuses=0xff
uno.bootloader.high_fuses=0xde
uno.bootloader.extended_fuses=0x05
uno.bootloader.path=optiboot
uno.bootloader.file=optiboot_atmega328.hex
uno.bootloader.unlock_bits=0x3F
uno.bootloader.lock_bits=0x0F
uno.build.mcu=atmega328p
uno.build.f_cpu=16000000L
uno.build.core=arduino
uno.build.variant=standard

##############################################################

atmega328.name=Arduino Duemilanove w/ ATmega328

atmega328.upload.protocol=arduino
atmega328.upload.maximum_size=30720
atmega328.upload.speed=57600

atmega328.bootloader.low_fuses=0xFF
atmega328.bootloader.high_fuses=0xDA
atmega328.bootloader.extended_fuses=0x05
atmega328.bootloader.path=atmega
atmega328.bootloader.file=ATmegaBOOT_168_atmega328.hex
atmega328.bootloader.unlock_bits=0x3F
atmega328.bootloader.lock_bits=0x0F

atmega328.build.mcu=atmega328p
atmega328.build.f_cpu=16000000L
atmega328.build.core=arduino
atmega328.build.variant=standard

##############################################################

diecimila.name=Arduino Diecimila or Duemilanove w/ ATmega168

diecimila.upload.protocol=arduino
diecimila.upload.maximum_size=14336
diecimila.upload.speed=19200

diecimila.bootloader.low_fuses=0xff
diecimila.bootloader.high_fuses=0xdd
diecimila.bootloader.extended_fuses=0x00
diecimila.bootloader.path=atmega
diecimila.bootloader.file=ATmegaBOOT_168_diecimila.hex
diecimila.bootloader.unlock_bits=0x3F
diecimila.bootloader.lock_bits=0x0F

diecimila.build.mcu=atmega168
diecimila.build.f_cpu=16000000L
diecimila.build.core=arduino
diecimila.build.variant=standard

##############################################################

nano328.name=Arduino Nano w/ ATmega328

nano328.upload.protocol=arduino
nano328.upload.maximum_size=30720
nano328.upload.speed=57600

nano328.bootloader.low_fuses=0xFF
nano328.bootloader.high_fuses=0xDA
nano328.bootloader.extended_fuses=0x05
nano328.bootloader.path=atmega
nano328.bootloader.file=ATmegaBOOT_168_atmega328.hex
nano328.bootloader.unlock_bits=0x3F
nano328.bootloader.lock_bits=0x0F

nano328.build.mcu=atmega328p
nano328.build.f_cpu=16000000L
nano328.build.core=arduino
nano328.build.variant=eightanaloginputs

##############################################################

nano.name=Arduino Nano w/ ATmega168

nano.upload.protocol=arduino
nano.upload.maximum_size=14336
nano.upload.speed=19200

nano.bootloader.low_fuses=0xff
nano.bootloader.high_fuses=0xdd
nano.bootloader.extended_fuses=0x00
nano.bootloader.path=atmega
nano.bootloader.file=ATmegaBOOT_168_diecimila.hex
nano.bootloader.unlock_bits=0x3F
nano.bootloader.lock_bits=0x0F

nano.build.mcu=atmega168
nano.build.f_cpu=16000000L
nano.build.core=arduino
nano.build.variant=eightanaloginputs

##############################################################

mega2560.name=Arduino Mega 2560 or Mega ADK

mega2560.upload.protocol=wiring
mega2560.upload.maximum_size=258048
mega2560.upload.speed=115200

mega2560.bootloader.low_fuses=0xFF
mega2560.bootloader.high_fuses=0xD8
mega2560.bootloader.extended_fuses=0xFD
mega2560.bootloader.path=stk500v2
mega2560.bootloader.file=stk500boot_v2_mega2560.hex
mega2560.bootloader.unlock_bits=0x3F
mega2560.bootloader.lock_bits=0x0F

mega2560.build.mcu=atmega2560
mega2560.build.f_cpu=16000000L
mega2560.build.core=arduino
mega2560.build.variant=mega

##############################################################

mega.name=Arduino Mega (ATmega1280)

mega.upload.protocol=arduino
mega.upload.maximum_size=126976
mega.upload.speed=57600

mega.bootloader.low_fuses=0xFF
mega.bootloader.high_fuses=0xDA
mega.bootloader.extended_fuses=0xF5
mega.bootloader.path=atmega
mega.bootloader.file=ATmegaBOOT_168_atmega1280.hex
mega.bootloader.unlock_bits=0x3F
mega.bootloader.lock_bits=0x0F

mega.build.mcu=atmega1280
mega.build.f_cpu=16000000L
mega.build.core=arduino
mega.build.variant=mega

##############################################################

leonardo.name=Arduino Leonardo
leonardo.upload.protocol=avr109
leonardo.upload.maximum_size=28672
leonardo.upload.speed=57600
leonardo.upload.disable_flushing=true
leonardo.bootloader.low_fuses=0xff
leonardo.bootloader.high_fuses=0xd8
leonardo.bootloader.extended_fuses=0xcb
leonardo.bootloader.path=caterina
leonardo.bootloader.file=Caterina-Leonardo.hex
leonardo.bootloader.unlock_bits=0x3F
leonardo.bootloader.lock_bits=0x2F
leonardo.build.mcu=atmega32u4
leonardo.build.f_cpu=16000000L
leonardo.build.vid=0x2341
leonardo.build.pid=0x8036
leonardo.build.core=arduino
leonardo.build.variant=leonardo

##############################################################

esplora.name=Arduino Esplora
esplora.upload.protocol=avr109
esplora.upload.maximum_size=28672
esplora.upload.speed=57600
esplora.upload.disable_flushing=true
esplora.bootloader.low_fuses=0xff
esplora.bootloader.high_fuses=0xd8
esplora.bootloader.extended_fuses=0xcb
esplora.bootloader.path=caterina
esplora.bootloader.file=Caterina-Esplora.hex
esplora.bootloader.unlock_bits=0x3F
esplora.bootloader.lock_bits=0x2F
esplora.build.mcu=atmega32u4
esplora.build.f_cpu=16000000L
esplora.build.vid=0x2341
esplora.build.pid=0x803C
esplora.build.core=arduino
esplora.build.variant=leonardo

##############################################################

micro.name=Arduino Micro
micro.upload.protocol=avr109
micro.upload.maximum_size=28672
micro.upload.speed=57600
micro.upload.disable_flushing=true
micro.bootloader.low_fuses=0xff
micro.bootloader.high_fuses=0xd8
micro.bootloader.extended_fuses=0xcb
micro.bootloader.path=caterina
micro.bootloader.file=Caterina-Micro.hex
micro.bootloader.unlock_bits=0x3F
micro.bootloader.lock_bits=0x2F
micro.build.mcu=atmega32u4
micro.build.f_cpu=16000000L
micro.build.vid=0x2341
micro.build.pid=0x8037
micro.build.core=arduino
micro.build.variant=micro

##############################################################

mini328.name=Arduino Mini w/ ATmega328

mini328.upload.protocol=arduino
mini328.upload.maximum_size=28672
mini328.upload.speed=115200

mini328.bootloader.low_fuses=0xff
mini328.bootloader.high_fuses=0xd8
mini328.bootloader.extended_fuses=0x05
mini328.bootloader.path=optiboot
mini328.bootloader.file=optiboot_atmega328-Mini.hex
mini328.bootloader.unlock_bits=0x3F
mini328.bootloader.lock_bits=0x0F

mini328.build.mcu=atmega328p
mini328.build.f_cpu=16000000L
mini328.build.core=arduino
mini328.build.variant=eightanaloginputs

##############################################################

mini.name=Arduino Mini w/ ATmega168

mini.upload.protocol=arduino
mini.upload.maximum_size=14336
mini.upload.speed=19200

mini.bootloader.low_fuses=0xff
mini.bootloader.high_fuses=0xdd
mini.bootloader.extended_fuses=0x00
mini.bootloader.path=atmega
mini.bootloader.file=ATmegaBOOT_168_ng.hex
mini.bootloader.unlock_bits=0x3F
mini.bootloader.lock_bits=0x0F

mini.build.mcu=atmega168
mini.build.f_cpu=16000000L
mini.build.core=arduino
mini.build.variant=eightanaloginputs

##############################################################

ethernet.name=Arduino Ethernet

ethernet.upload.protocol=arduino
ethernet.upload.maximum_size=32256
ethernet.upload.speed=115200

ethernet.bootloader.low_fuses=0xff
ethernet.bootloader.high_fuses=0xde
ethernet.bootloader.extended_fuses=0x05
ethernet.bootloader.path=optiboot
ethernet.bootloader.file=optiboot_atmega328.hex
ethernet.bootloader.unlock_bits=0x3F
ethernet.bootloader.lock_bits=0x0F

ethernet.build.variant=ethernet
ethernet.build.mcu=atmega328p
ethernet.build.f_cpu=16000000L
ethernet.build.core=arduino

##############################################################

fio.name=Arduino Fio

fio.upload.protocol=arduino
fio.upload.maximum_size=30720
fio.upload.speed=57600

fio.bootloader.low_fuses=0xFF
fio.bootloader.high_fuses=0xDA
fio.bootloader.extended_fuses=0x05
fio.bootloader.path=arduino:atmega
fio.bootloader.file=ATmegaBOOT_168_atmega328_pro_8MHz.hex
fio.bootloader.unlock_bits=0x3F
fio.bootloader.lock_bits=0x0F

fio.build.mcu=atmega328p
fio.build.f_cpu=8000000L
fio.build.core=arduino
fio.build.variant=eightanaloginputs

##############################################################

bt328.name=Arduino BT w/ ATmega328

bt328.upload.protocol=arduino
bt328.upload.maximum_size=28672
bt328.upload.speed=19200
bt328.upload.disable_flushing=true

bt328.bootloader.low_fuses=0xff
bt328.bootloader.high_fuses=0xd8
bt328.bootloader.extended_fuses=0x05
bt328.bootloader.path=bt
bt328.bootloader.file=ATmegaBOOT_168_atmega328_bt.hex
bt328.bootloader.unlock_bits=0x3F
bt328.bootloader.lock_bits=0x0F

bt328.build.mcu=atmega328p
bt328.build.f_cpu=16000000L
bt328.build.core=arduino
bt328.build.variant=eightanaloginputs

##############################################################

bt.name=Arduino BT w/ ATmega168

bt.upload.protocol=arduino
bt.upload.maximum_size=14336
bt.upload.speed=19200
bt.upload.disable_flushing=true

bt.bootloader.low_fuses=0xff
bt.bootloader.high_fuses=0xdd
bt.bootloader.extended_fuses=0x00
bt.bootloader.path=bt
bt.bootloader.file=ATmegaBOOT_168.hex
bt.bootloader.unlock_bits=0x3F
bt.bootloader.lock_bits=0x0F

bt.build.mcu=atmega168
bt.build.f_cpu=16000000L
bt.build.core=arduino
bt.build.variant=eightanaloginputs

##############################################################

LilyPadUSB.name=LilyPad Arduino USB
LilyPadUSB.upload.protocol=avr109
LilyPadUSB.upload.maximum_size=28672
LilyPadUSB.upload.speed=57600
LilyPadUSB.upload.disable_flushing=true
LilyPadUSB.bootloader.low_fuses=0xff
LilyPadUSB.bootloader.high_fuses=0xd8
LilyPadUSB.bootloader.extended_fuses=0xce
LilyPadUSB.bootloader.path=caterina-LilyPadUSB
LilyPadUSB.bootloader.file=Caterina-LilyPadUSB.hex
LilyPadUSB.bootloader.unlock_bits=0x3F
LilyPadUSB.bootloader.lock_bits=0x2F
LilyPadUSB.build.mcu=atmega32u4
LilyPadUSB.build.f_cpu=8000000L
LilyPadUSB.build.vid=0x1B4F
LilyPadUSB.build.pid=0x9208
LilyPadUSB.build.core=arduino
LilyPadUSB.build.variant=leonardo

##############################################################

lilypad328.name=LilyPad Arduino w/ ATmega328

lilypad328.upload.protocol=arduino
lilypad328.upload.maximum_size=30720
lilypad328.upload.speed=57600

lilypad328.bootloader.low_fuses=0xFF
lilypad328.bootloader.high_fuses=0xDA
lilypad328.bootloader.extended_fuses=0x05
lilypad328.bootloader.path=atmega
lilypad328.bootloader.file=ATmegaBOOT_168_atmega328_pro_8MHz.hex
lilypad328.bootloader.unlock_bits=0x3F
lilypad328.bootloader.lock_bits=0x0F

lilypad328.build.mcu=atmega328p
lilypad328.build.f_cpu=8000000L
lilypad328.build.core=arduino
lilypad328.build.variant=standard

##############################################################

lilypad.name=LilyPad Arduino w/ ATmega168

lilypad.upload.protocol=arduino
lilypad.upload.maximum_size=14336
lilypad.upload.speed=19200

lilypad.bootloader.low_fuses=0xe2
lilypad.bootloader.high_fuses=0xdd
lilypad.bootloader.extended_fuses=0x00
lilypad.bootloader.path=lilypad
lilypad.bootloader.file=LilyPadBOOT_168.hex
lilypad.bootloader.unlock_bits=0x3F
lilypad.bootloader.lock_bits=0x0F

lilypad.build.mcu=atmega168
lilypad.build.f_cpu=8000000L
lilypad.build.core=arduino
lilypad.build.variant=standard

##############################################################

pro5v328.name=Arduino Pro or Pro Mini (5V, 16 MHz) w/ ATmega328

pro5v328.upload.protocol=arduino
pro5v328.upload.maximum_size=30720
pro5v328.upload.speed=57600

pro5v328.bootloader.low_fuses=0xFF
pro5v328.bootloader.high_fuses=0xDA
pro5v328.bootloader.extended_fuses=0x05
pro5v328.bootloader.path=atmega
pro5v328.bootloader.file=ATmegaBOOT_168_atmega328.hex
pro5v328.bootloader.unlock_bits=0x3F
pro5v328.bootloader.lock_bits=0x0F

pro5v328.build.mcu=atmega328p
pro5v328.build.f_cpu=16000000L
pro5v328.build.core=arduino
pro5v328.build.variant=standard

##############################################################

pro5v.name=Arduino Pro or Pro Mini (5V, 16 MHz) w/ ATmega168

pro5v.upload.protocol=arduino
pro5v.upload.maximum_size=14336
pro5v.upload.speed=19200

pro5v.bootloader.low_fuses=0xff
pro5v.bootloader.high_fuses=0xdd
pro5v.bootloader.extended_fuses=0x00
pro5v.bootloader.path=atmega
pro5v.bootloader.file=ATmegaBOOT_168_diecimila.hex
pro5v.bootloader.unlock_bits=0x3F
pro5v.bootloader.lock_bits=0x0F

pro5v.build.mcu=atmega168
pro5v.build.f_cpu=16000000L
pro5v.build.core=arduino
pro5v.build.variant=standard

##############################################################

pro328.name=Arduino Pro or Pro Mini (3.3V, 8 MHz) w/ ATmega328

pro328.upload.protocol=arduino
pro328.upload.maximum_size=30720
pro328.upload.speed=57600

pro328.bootloader.low_fuses=0xFF
pro328.bootloader.high_fuses=0xDA
pro328.bootloader.extended_fuses=0x05
pro328.bootloader.path=atmega
pro328.bootloader.file=ATmegaBOOT_168_atmega328_pro_8MHz.hex
pro328.bootloader.unlock_bits=0x3F
pro328.bootloader.lock_bits=0x0F

pro328.build.mcu=atmega328p
pro328.build.f_cpu=8000000L
pro328.build.core=arduino
pro328.build.variant=standard

##############################################################

pro.name=Arduino Pro or Pro Mini (3.3V, 8 MHz) w/ ATmega168

pro.upload.protocol=arduino
pro.upload.maximum_size=14336
pro.upload.speed=19200

pro.bootloader.low_fuses=0xc6
pro.bootloader.high_fuses=0xdd
pro.bootloader.extended_fuses=0x00
pro.bootloader.path=atmega
pro.bootloader.file=ATmegaBOOT_168_pro_8MHz.hex
pro.bootloader.unlock_bits=0x3F
pro.bootloader.lock_bits=0x0F

pro.build.mcu=atmega168
pro.build.f_cpu=8000000L
pro.build.core=arduino
pro.build.variant=standard

##############################################################

atmega168.name=Arduino NG or older w/ ATmega168

atmega168.upload.protocol=arduino
atmega168.upload.maximum_size=14336
atmega168.upload.speed=19200

atmega168.bootloader.low_fuses=0xff
atmega168.bootloader.high_fuses=0xdd
atmega168.bootloader.extended_fuses=0x00
atmega168.bootloader.path=atmega
atmega168.bootloader.file=ATmegaBOOT_168_ng.hex
atmega168.bootloader.unlock_bits=0x3F
atmega168.bootloader.lock_bits=0x0F

atmega168.build.mcu=atmega168
atmega168.build.f_cpu=16000000L
atmega168.build.core=arduino
atmega168.build.variant=standard

##############################################################

atmega8.name=Arduino NG or older w/ ATmega8

atmega8.upload.protocol=arduino
atmega8.upload.maximum_size=7168
atmega8.upload.speed=19200

atmega8.bootloader.low_fuses=0xdf
atmega8.bootloader.high_fuses=0xca
atmega8.bootloader.path=atmega8
atmega8.bootloader.file=ATmegaBOOT-prod-firmware-2009-11-07.hex
atmega8.bootloader.unlock_bits=0x3F
atmega8.bootloader.lock_bits=0x0F

atmega8.build.mcu=atmega8
atmega8.build.f_cpu=16000000L
atmega8.build.core=arduino
atmega8.build.variant=standard

##############################################################

robotControl.name=Arduino Robot Control
robotControl.upload.protocol=avr109
robotControl.upload.maximum_size=28672
robotControl.upload.speed=57600
robotControl.upload.disable_flushing=true
robotControl.bootloader.low_fuses=0xff
robotControl.bootloader.high_fuses=0xd8
robotControl.bootloader.extended_fuses=0xcb
robotControl.bootloader.path=caterina-Arduino_Robot
robotControl.bootloader.file=Caterina-Robot-Control.hex
robotControl.bootloader.unlock_bits=0x3F
robotControl.bootloader.lock_bits=0x2F
robotControl.build.mcu=atmega32u4
robotControl.build.f_cpu=16000000L
robotControl.build.vid=0x2341
robotControl.build.pid=0x8038
robotControl.build.core=robot
robotControl.build.variant=robot_control

##############################################################

robotMotor.name=Arduino Robot Motor
robotMotor.upload.protocol=avr109
robotMotor.upload.maximum_size=28672
robotMotor.upload.speed=57600
robotMotor.upload.disable_flushing=true
robotMotor.bootloader.low_fuses=0xff
robotMotor.bootloader.high_fuses=0xd8
robotMotor.bootloader.extended_fuses=0xcb
robotMotor.bootloader.path=caterina-Arduino_Robot
robotMotor.bootloader.file=Caterina-Robot-Motor.hex
robotMotor.bootloader.unlock_bits=0x3F
robotMotor.bootloader.lock_bits=0x2F
robotMotor.build.mcu=atmega32u4
robotMotor.build.f_cpu=16000000L
robotMotor.build.vid=0x2341
robotMotor.build.pid=0x8039
robotMotor.build.core=robot
robotMotor.build.variant=robot_motor


##############################################################

atmega328_384_8.name=ATmega328 Optiboot @ 38,400baud w/ 8MHz Int. RC Osc.

atmega328_384_8.upload.protocol=arduino
atmega328_384_8.upload.maximum_size=30720
atmega328_384_8.upload.speed=38400

atmega328_384_8.bootloader.low_fuses=0xCF
atmega328_384_8.bootloader.high_fuses=0xD6
atmega328_384_8.bootloader.extended_fuses=0xFD
atmega328_384_8.bootloader.path=optiboot
atmega328_384_8.bootloader.file=optiboot_atmega328_384_8.hex
atmega328_384_8.bootloader.unlock_bits=0x3F
atmega328_384_8.bootloader.lock_bits=0x0F

atmega328_384_8.build.mcu=atmega328p
atmega328_384_8.build.f_cpu=8000000L
atmega328_384_8.build.core=arduino
atmega328_384_8.build.variant=standard


##############################################################

atmega328_8xt.name=ATmega328 Optiboot @ 115,200baud w/ 8MHz Ext. Osc.

atmega328_8xt.upload.protocol=arduino
atmega328_8xt.upload.maximum_size=30720
atmega328_8xt.upload.speed=38400

atmega328_8xt.bootloader.low_fuses=0xCF
atmega328_8xt.bootloader.high_fuses=0xD6
atmega328_8xt.bootloader.extended_fuses=0xFD
atmega328_8xt.bootloader.path=optiboot
atmega328_8xt.bootloader.file=optiboot_atmega328_8xt.hex
atmega328_8xt.bootloader.unlock_bits=0x3F
atmega328_8xt.bootloader.lock_bits=0x0F

atmega328_8xt.build.mcu=atmega328p
atmega328_8xt.build.f_cpu=8000000L
atmega328_8xt.build.core=arduino
atmega328_8xt.build.variant=standard



